ISUP SSC Configuration Bytes (ITU)

Byte | Description | Value
--- | --- | ---
0x01 | Note Used |
0x02 | SGM indication to host | 0 Concatenate Message with SGM and report to host. 1 (default) Send Separate SGMindication (event: 0x38, comp: 0x0F)
0x03 | Not used |
0x04 | Outgoing Segmentation length limit | 1 (default) (MSB) This makes it 0x104 which is equal to 260 octets.
0x05 |  | 4 (default) (LSB)

In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.
Most Significant Bit
Least Significant Bit