0x05FA Card Object

Use this TLV in the Generic Card Configure message to identify the card to be configured. The card uses this information to verify that the message is intended for it.

Byte | Description
0, 1 | Tag: 0x05FA - Card Object
2, 3 | Length: 0x0004
4, 5 | Value[0, 1]: Card Type ID Refer to the Card Population Query 0x0007 message for a list of the card types.
6, 7 | Value[2, 3]: Object ID 0x0000 - General Card Configuration 0x0001 - Conferencing Parameters 0x0003 - Alarm Configuration (Used in Generic Card Query message only) 0x0004 - DSP Series 2 Fax Parameters Query 0x0005 - Echo Cancel 0x0006 - PVD/AMD Parameters 0x0007 - Dial Pulse Detection Parameters

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor