Purpose

This section includes a PPL Config Byte and PPL Event for the PPL Component MTP2 IAC.

Configuration Byte

Byte | Description | Value
--- | --- | ---
0x10 | Raw LSSU transmitted to adjacent Node The PPL Event Indications for the LSSU received will not contain the IAC component ID. | 0x00=Disable (default) 0x01=Enable the PPL Event Indication containing the LSSU transmitted to the adjacent Node.

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
A programmable software component that uses PPL state machines that can be modified with the PPL Tool.
Message Transfer Part level 2 - data link level