0x0282 PPL Event Notification Mask

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x0282
2, 3 | Length 0x0004
4-7 | Value[0-3] 32 bit mask with each bit selects specific PPL Event Indication. Bit 0 - Media changed via the RE-INVITE message (Event ID 0x001E) Bit 1 - 200 OK Received (Event ID 0x0020) Bit 2 - 183 received (Event ID 0x001F) Bit 3 - 180 received (Event ID 0x0024) Bit 4 - ACK with SDP (Delayed Media) Bit 5 - PRACK received (Event ID 0x002A) Bit 6 - On server side, report INFO message received (Event ID 0x002C). On client side, report the response received for INFO message sent (Event ID 0x002D). Bit 7 - 182 Received (Event ID 0x002E) Bit 8 - Options message received. (Event ID 0x002F) Bit 9 - 181 Received (Event ID 0x0030) Bit 10 - 422 Received (Event ID 0x0031) Bits 8-31. Undefined. Bits 0, 1, 2, 4, 5, and 10 are enabled by default. All other bits are disabled by default.

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
See Programmable Protocol Language.
Positive acknowledgment to a message