You are here: CSP Developer’s Guide: Overview > 8 DSP Series 2 Cards Product Description > DSP Alarms

DSP Alarms

DSP Related Alarms shows the alarms reported in the Alarm 0x00B9 message that relate to DSP functionality. See the message for details.

Table 8-6 DSP Related Alarms

Alarm Type | Severity | Alarm Number/Name
--- | --- | ---
General (0x01) | Major | 0x06 - DSP Resource Blocked
0x07 - DSP Resource Function Type Not Configured
0x08 - DSP Resource Management Inconsistent
0x3F - Insufficient Resource Points for DSP Function
00x40 - DSP Request Queued Due to DSP Series 2 CPU Overload Level 2
Informational | 0x34 - DSP CPA Configuration Conflict
Card (0x02) | Major | 0x41 - NFS Server Mounting Error
0x43 - DSP Series 2 File Space Out of Memory
0x45 - NFS Traffic Threshold Major Alarm
0x46 - DSP Series 2 TFTP Communications Error
0x47 - NFS Read Error
0x48 - NFS Write Error
0x4B - NFS Server Unmount Error
0x4C - NFS Open File Error
Minor | 0x44 - NFS Traffic Minor Threshold Alarm
0x42 - DSP Series 2 File Space Low
Card (cont.) | Informational | 0x49 - Vocabulary Index File Read
0x4A - NFS Server Unmounted
0x40 - NFS Server Mounted Successfully
Channel (0x04) | Major | 0x0A - DSP Resource Wait Timeout
DSP SIMM (0x05) | Major | 0x04 - Recorded Announcement Download Inconsistency
0x05 - Recorded Announcement ID Inconsistency (on same card)
0x08 - Recorded Announcement File System Conversion Failure
0x09 - Recorded Announcement File System Timeout
0x0C - Recorded Announcement Defragmentation Failure
Informational | 0x01 - DSP SIMM Taken Out of Service
0x03 - Recorded Announcement Erase Complete
0x06 - Recorded Announcement Download Ready
0x07 - Recorded Announcement File System Conversion Success
0x0B - Recorded Announcement Defragmentation Success
0x0D - Recorded Announcement Single Deletion Complete
0x0E - Recorded Announcement Need Defragmentation
DSP (0x06) | Major | 0x01 - DSP Out of Service
0x03 - DSP Playback Underrun
0x04 - DSP Record Overrun
0x05 - DSP Temporary Storage Minor Alarm
0x06 - DSP Temporary Storage Full
0x08 - DSP Chip Reset
Informational | 0x02 - Resources Exceed Limit
0x07 - DSP Points Exceed Limit

Digital Signal Processor