0x005E Resource Client ID

Used in:
Route Control message

Byte | Description
0, 1 | Tag 0x005E
2, 3 | Length 0x0008
4,5 | Value[0, 1] Alias ID (MSB, LSB) 0x0002 = V5 Client
6,7 | Value[2,3] Reserved
8-11 | Value[4-7] Client ID: V5 ID

Most Significant Bit
Least Significant Bit
In SIP, an application program that sends SIP requests (See also Session Initiation Protocol). Clients may or may not interact directly with a person. Users agents and proxies contain clients (and servers).