L3P System Management Component PPL Timers (0x0090)

When specifying new timer values, remember that all PPL Timers are specified in 10 ms increments. For example, a PPL timer for 4 seconds is specified as 4000 (decimal, 400 x 10 ms = 4 seconds), which is the hexadecimal value of (0x190).

Timer ID | Description | Value (default)
--- | --- | ---
0x01 | Waiting for MDU Control (restart acknowledge) from all PSTN protocol State Machines | 100 seconds
0x02 | Waiting for MDU Control (restart complete) from Control Data Link | 120 seconds
0x03 | Waiting for MDL Establish Confirm or MDL Establish Indication from Control Data Link | 15 seconds
0x04 | Waiting for MDL Establish Confirm or MDL Establish Indication from Control Data Link | 60 seconds
0x05 | Waiting for MDL Establish Confirm or MDL Establish Indication from PSTN Data Link | 25 seconds
0x06 | Waiting for MDL Establish Confirm or MDL Establish Indication from Link Control Data Link | 15 seconds
0x07 | Waiting for MDL Establish Confirm or MDL Establish Indication from Link Control Data Link | 60 seconds
0x08 | Waiting for MDL Establish Confirm or MDL Establish Indication from BCC Data Link | 15 seconds
0x09 | Waiting for MDU Control (Unblock all relevant ports accepted) | 20 seconds
0x0A | Waiting for MDU Control (Unblock all relevant ports accepted) | 10 seconds

See Programmable Protocol Language.
Public Switched Telephone Network
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.