0x0275 Local Registration Enable/Disable

Use this TLV to enable or disable the acceptance of local registrations within the CSP.

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x0275
2, 3 | Length 0x0001
4 | Value[0] Local Registration Enable/Disable 0x00 Disable local storage of registrations 0x01 (Default) Store up to 2048 SIP phone registrations locally in the CSP.

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Session-Initiation Protocol. A signaling protocol used for establishing sessions in an IP network. A session could be a simple, two-way telephone call, or it could be a collaborative multi-media conference session.