L3P SSUTR2 PPL Event Requests

Event ID | Event
--- | ---
0x01 | Send ACF (Alerting)
0x02 | Send ECH (Call failure message)
0x03 | Send DEG (General Setup Request)
0x04 | Send Call Unsuccessful (Call unsuccessful signal)
0x05 | Send RIU (Answer)
0x06 | Send RAU (Clear Back)
0x07 | Send NRP (Reanswer)
0x08 | Send MSS/MSA (Subsequent address)
0x09 | Send IFG (General setup information)
0x0D | Send BLOA (manual incoming blocking)
0x0E | Send BLOA clear (unblock incoming)
0x13 | Circuit reset request
0x14 | Circuit group reset request
0x64 | Send CCD (Manual Outgoing Continuity Recheck)
0x65 | Stop CCD (Stop Outgoing Continuity Recheck)
0x66 | Send End to End Message MUU/MCE
0x67 | Local BLOF
0x68 | Local BLOD (manual outgoing blocking)
0x69 | Local BLOD (manual outgoing blocking) clear
0x6A | Local BLOS (Blocking due to internal system fault)
0x6B | Local BLOS (Blocking due to internal system fault) clear
0x6C | Send TAX
0x6D | Send CHT
0x6E | Send ITX
0x6F | Local BLOF clear