You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Assign Logical Node ID 0x0010

Assign Logical Node ID 0x0010

SwitchKit Name

AssignNode

Type

EXS API and SwitchKit API message

Description

Assign Logical Node ID 0x0010

Use this message to assign a logical node ID to a CSP that is a node in a multi-node system.

If the node has an EXNET-ONE card installed or if you plan to have an EXNET-ONE card installed, you must assign the node ID at configuration.

The default logical node ID for a stand-alone CSP is 0xFF. To specify the node that you are assigning a logical ID, you use its physical node ID (serial number).

NOTE: For SwitchKit, DO NOT use the XL_AssignNode message with EXS SwitchKit. XL_AssignNode is obsolete with the introduction of SK_AddLLCNode.

Sent by

Host

Example Message (SwitchKit Socket Log Output)

In the following socket log output/example message, the host assigns logical node ID 01 to the physical node 0000 23AC for the first time:

00 0D 00 10 00 00 FF 00 01 10 05 00 00 23 AC 01

SwitchKit Code

Configuration

AssignNode (

Node = integer,

PhysicalNode = integer,

LogicalNode = integer);

C Structure

typedef struct {

BaseFields Base;

int PhysicalNode;

UBYTE LogicalNode;

} XL_AssignNode;

C++ Class

class XLC_AssignNode : public XLC_OutboundMessage {

public:

int getPhysicalNode() const;

void setPhysicalNode(int x);

UBYTE getLogicalNode() const;

void setLogicalNode(UBYTE x);

UBYTE getISUPRemCon() const;

void setISUPRemCon(UBYTE x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x00NN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x0010) | 3, 4 | Message Type (0x0010)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Current Logical Node ID If assigning for first time, byte 7 is 0xFF. | 7 | Logical Node ID
: | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status (MSB, LSB) 0x007F Software Module Locked See also the Common Response Status Values chapter
Number of AEs to follow
AEs 0x10 Logical/Physical Node
: | ISUP Remote Control 0x00 Disable ISUP Remote Control (Default) 0x01 Enable ISUP Remote Control |  |
: | Checksum | 10 | Checksum

Excel's open architecture, proprietary, 1.3 Gbps fiber optic network using a packet-based protocol.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit
See Integrated Services Digital Network User Part.