0x01 Add Virtual Card

Used in:
Virtual Card Configure message

Byte | Description
0 | Tag 0x01 Add Virtual Card
1 | Length 0x02
2 | Value[0] Slot Number 0x40- 0x5F
3 | Value[1] Card Type 0xD2 Virtual T1 16 Span 0xD5 Virtual E1/J1 16 Span 0x80 Virtual 32 Span VDAC-ONE or IP Media Series 2

Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.
A digital communications link - voice, data, and video at a 2.048 Mbps rate; 30B/2D or 31B/1D (ISDN); non-North American version of T1.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.