VoIP

0x009C VDAC-ONE VoIP Component*

0x009F - IP Network Interface Series 2 VoIP Component *

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.