SIP

Comp ID | Comp. Name | PPL Assign | PPL Audit Config. | PPL Audit Query | PPL Config. | PPL Data Query | PPL Event Request/ Indication | PPL Timer Config.
--- | --- | --- | --- | --- | --- | --- | --- | ---
0x00A7 | SIP UA | N/A | 0x7F * 0x0D ** | N/A
* Used for registration events ** Used for call control events For more information, refer to PPL Information: SIP UA 0xA7 in the SIP Software chapter in the Developer’s Guide: Internet Protocol. |

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
Session-Initiation Protocol. A signaling protocol used for establishing sessions in an IP network. A session could be a simple, two-way telephone call, or it could be a collaborative multi-media conference session.