You are here: CSP Hardware Product Descriptions > 4 Common Channel Signaling Cards > CCS I/O Redundancy Cable Assembly - Part Nos. 64012301/ 164012301

CCS I/O Redundancy Cable Assembly - Part Nos. 64-0123-01/ 164-0123-01

Description

The CCS I/O Redundancy cable serves as an independent HDLC link for redundancy between the adjacent CCS I/O cards.

Specifications

The CCS I/O redundant cable assembly is designed to the following specifications.

Parameter | Specification
--- | ---
Length | 10 in.
Connectors | DB-9 male

Related Product

The product related to the CCS I/O Redundancy cable assembly is listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
CCS I/O Card | CSP-CCS-1001 | CSP-CCS-1001R

Cable Assembly Connections

The CCS I/O Redundancy cable assembly is connected as shown in the diagram below.

See Common Channel Signaling.