0x2964 SIP MIME Information

Used in:
0x0033 NPDI Universal ICB in:
Route Control message
Outseize Control message
Release Channel with Data
Connect with Data
Channel Released with Data
Request for Service with Data message
PPL Event Request message
PPL Event Indication message

Byte | Description
0, 1 | Tag 0x2964
2, 3 | Length Variable (Maximum of 780 bytes)

Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.
Outgoing call setup during real-time call processing on a specific channel.
See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.