L3 Call Reference Configuration Bytes

These values are for connection to the Lucent 4ESS. See L3 Default Settings per Connection Type for variations from the defaults shown here for other Connection Types.

Asterisks (*) denote default values.

Byte | Description | Values
--- | --- | ---
0x01 | Connect Ack Option (Send a Connect Ack in response to a Connect.) | 0x00 = Disabled (False) * 0x01 = Enabled (True)
0x02 | Reserved | None
0x03 | Status Enquiry Option (Send a Status Inquire message rather than a Status message when receiving an invalid message in the NULL state.) | * 0x00 = Disabled 0x01 = Enabled
0x04 | The accepted received Bearer Capability Bit Mask. | 0x01 = Voice 0x02 = 3.1 KHz Audio * 0x03 = Voice and 3.1 KHz Audio 0x04 = Unrestricted 56K 0x08 = Unrestricted 64K 0x10 = Restricted 64K 0x20 = 384 K 0x40 = 7.1 KHz Audio
0x05 | Channel ID encoding of extension bit (octet 5 in channel ID IE) | * 0x00 = Extension (Ext.) bit set 0x01 = Ext. bit cleared
0x06 | Call Proceeding Option (send call proceeding once the call is answered, not automatically after receiving SETUP) | * 0x00 = Disabled 0x01 = Enabled
0x07 | Number of SETUP resends (after T303 expiry) NOTE: Not applicable for JATE variant | 0x01 = Resend
0x08 | Acceptable Information transfer rate. In BCC IE for incoming calls. | 0x01 * = CIRC (Circuit) mode 64K 0x02 = CIRC mode 2_64K 0x04 = CIRC mode 384K 0x08 = CIRC mode 1563K 0x10 = CIRC mode 1920K 0x20 = CIRC mode MULTIRATE
0x09 | Send CONNECT ACK indication to the host. | 0x00 = Disabled (default) 0x01 = Enabled
0x0A | Call Reference Allocation can be set to (FALSE) which always takes the next value in the list, or (TRUE) which takes the first unused value always searching from the start of the list. | 0x00 = False (Default) 0x01 = True
0x22 | Number of re-transmission of Status Enquiry Request. | *0x00
QSIG/PSS1 only
0x23 | Send Unexpected Segmented Message to host | 0x00 = Disabled *0x01 = Enabled
0x24 | Send Segmentation Failure - Wrong or Unexpected Segmented Message to host | 0x00 = Disabled *0x01 = Enabled
Euro-ISDN Only
0x08 | Connect ACK to host | 0x00* = Do Not Send
0x09 | STATUS to host | 0x00* = Do Not Send
0x0B | Glare Control | 0x00* = Drop Outgoing

Japan Approvals Institute for Telecommunications Equipment
Positive acknowledgment to a message
See Integrated Services Digital Network.