You are here: CSP Hardware Product Descriptions > 6 Resource Cards > Dialogic® Multi-Function Media I/O Card - CSP-BIO-1000/ CSP-BIO-1000R

Dialogic® Multi-Function Media I/O Card - CSP-BIO-1000/
CSP-BIO-1000R

Description

The Dialogic® Multi-Function Media I/O card is required to operate the IP Network Interface Series 2 and DSP Series 2 cards. The Multi-Function Media I/O card connects to the IP Network Interface Series 2 and DSP Series 2 cards through the chassis midplane.

Ethernet Ports

The Multi-Function Media I/O card provides three external 100Base-T (100 Mbps) Ethernet ports that can be used for redundancy.

Placement

The Multi-Function Media I/O card resides in the rear card slot of a CSP 2090, CSP 2110, or CSP 2040 chassis directly behind the corresponding IP Network Interface Series 2/3 or DSP Series 2 card.

Configuration Information

The part number, serial number, model number, and revision are located on the back of the board.

Specifications

The Multi-Function Media I/O card is designed to the following electrical, physical, and environmental specifications.

Electrical | Specification
--- | ---
Supply Voltage, Vcc | 5.00V
Supply Current, Vcc @ 5.0V | 1.0A (typical)

Physical | Specification
--- | ---
Height | 318.5 mm (12.54 in.)
Depth | 105.2 mm (4.14 in)
Width | 19.7 mm (0.775 in.)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) @ 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) @ 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 m (13,123 ft.)

Related Products

The products related to the Multi-Function Media I/O card are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
IP Network Interface Series 2 with one VoIP module | EXS-VDC-1200 | EXS-VDC-1200R
IP Network Interface Series 2 with two VoIP modules | EXS-VDC-1220 | EXS-VDC-1220R
IP Network Interface Series 3 with one VoIP module | N/A | CSP-IPN-3100R
IP Network Interface Series 3 with two VoIP modules | N/A | CSP-IPN-3200R
DSP Series 2 with one module | CSP-DSP 1310 | CSP-DSP 1310R
DSP Series 2 with two modules | CSP-DSP 1320 | CSP-DSP 1320R

Front and Side Views

The front view shows the LEDs, push button switch, and Ethernet connectors.

Controls and Indicators

The table below describes the LEDs as shown in the front view of the Multi-Function Media I/O card.

Fault, Hreset LEDs/Reset Push Button | Color/Status | Description
--- | --- | ---
Fault | Off | Reserved
Hreset | Green | Indicates the I/O card is being reset.
Reset | Initiates a reset of the I/O card.
Ethernet LEDs | Color/Status | Description
Activity | Green | Indicates both RX (receive) and TX (transmit) activity (20ms on time)
Off | Indicates no RX or TX activity
Col/FD (Collision/Duplex) | Green | Flashes when collision occurs in half duplex mode (20ms on time) Continuous indication when in full duplex mode Flashes (10 Hz) during continuous collisions
Off | Indicates no collisions
LNK (Link) | Green | Flashes during auto-negotiation Continuous indication when a link is established Continuously flashes during network misconfiguration
Off | Indicates loopback
100M (Speed) | Yellow | Indicates 100Base-T (100 Mbps) link established
Flashes (0.4 sec.) with no link established
Off | 10Base-T (10 Mbps) link not supported

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Digital Signal Processor
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Hertz