0x15 DASS2/DPNSS Raw Data

The DASS2/DPNSS Raw Data ICB is a Raw DASS2/DPNSS frame that starts at the message/group octet (it does not include the address and control octets).

Used in:
Route Control message
Outseize Control message

ICB Type | 0x02 (Data)
ICB ID | 0x15
Data Length | Variable
Data[0] | Raw DASS2/DPNSS Message/Group Octet
Data[1] | Remaining DASS2/DPNSS Frame

See Information Control Block.
Outgoing call setup during real-time call processing on a specific channel.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.