Purpose

This section includes PPL Config Bytes, all PPL Event Indications, and Timer information for the PPL Component SSUTR2 CPC, a variant of TUP CPC.

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
A programmable software component that uses PPL state machines that can be modified with the PPL Tool.
Telephone User Part