You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > DSP Service Cancel 0x00BE

DSP Service Cancel 0x00BE

SwitchKit Name

DSPServiceCancel

Type

EXS API and SwitchKit API message

Description

DSP Service Cancel 0x00BE

Use this message to cancel a DSP Service.

Sent by

Host

SwitchKit Code

C Structure

typedef struct {

unsigned short Span;

UBYTE Channel;

UBYTE ServiceType;

UBYTE reserved48[222];

} XL_DSPServiceCancel;

C++ Class

class XLC_DSPServiceCancel : public XLC_OneChannelOutbound {

public:

unsigned short getSpan() const;

void setSpan(unsigned short x);

UBYTE getChannel() const;

void setChannel(UBYTE x);

UBYTE getServiceType() const;

void setServiceType(UBYTE x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x00BE) | 3, 4 | Message Type (0x00BE)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status MSB, LSB
10 | Checksum
Number of AEs
AE 0x0D Channel
| Service Type 0x01 DTMF Receiver 0x02 Energy Detection 0x03 CPA Receiver 0x04 Coin Tone Receiver 0x05 CPA 2100 Hz Receiver 0x14 DTMF and Dial Pulse Receiver 0x15 Dial Pulse Receiver 0x16 DTMF and Dial Pulse Receiver with Termination of Tone/Announcement 0x17 Dial Pulse Receiver with Termination of Tone/Announcement 0x81 DTMF Receiver, Matrix ( Based RFC 2833 Collection) 0xC1 DTMF Receiver, Matrix ( Based on SUBSRIBE/NOTIFY) 0xE1 DTMF Receiver with Termination of Tone/Announcement
: | Checksum

Digital Signal Processor
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit
Hertz