L3 B Channel Control Configuration Bytes

Byte | Description | Values
--- | --- | ---
0x01 | Channel ID encoding of extension bit | * 0x00 = Ext. bit set 0x01 = Ext. bit cleared
0x02 | Enable support for sub-configured interface | 0x00 = Disabled (Default) 0x01 = Enabled
0x03 | Sending the indication from BSS to host reporting the B channel state | 0x00 - Disable send Indications (Default) 0x01 - Enable Send Indications