0x0A Socket Status

Used in:
IP Socket Status Report message

Byte | Description
0 | Tag 0x0A Socket Status
1 | Length 0x03
2 | Value[0] 0x00 Module (0xFF = Main Board)
3 | Value[1] 0x01-0x02 Socket ID
4 | Value[2] Socket Status 0x00 Socket is not connected, but allow for traffic when connected 0x01 Socket is connected. Allow for Traffic 0x02 Socket is not connected. Prohibit Traffic.

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.