0x027C Min-SE Interval

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Use this TLV to set the Min-SE header field (in seconds) which conveys the minimum allowed value for the session timer. The Min-SE Internal has to be less than the Session Interval. The maximum value is 0x7F FF FF FE.

Byte | Description
0, 1 | Tag 0x027C
2, 3 | Length 0x0004
4-7 | Value[0] Variable 300 (5 minutes) (Default) 0x00 00 01 2C

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.