You are here: CSP Developer’s Guide: Internet Protocol > 3 IP Network Interface Series 2 Card > Sample Route Control / Resource Attribute Configure

Sample Route Control / Resource Attribute Configure

The Route Control message below establishes a one-way listen only connection:

00 43 00 e8 00 00 ff \' Header

00 01 29 02 ff fe \ ' Router AIB

03 \ ' ICB count

03 00 33 00 12 00 02 27 92 00 04 0a 0a 24 15 27 93 00 04 00 00 00 01 \ ' Universal ICB

02 1e 13 00 03 00 13 00 02 00 06 00 06 00 02 00 01 00 0f 00 01 0b \ ' Router ICB

02 1e 07 00 01 01 db 00 01 01 \ ' Connection Mode TLV

The Route Control message below establishes a one-way talk only connection:

00 67 00 e8 00 00 ff \' Header

00 01 29 02 ff fe \ ' Router AIB

03 \ ' ICB count

03 00 33 00 22 00 04 27 92 00 04 0a 0a 24 15 27 93 00 04 00 00 00 01 \

' Universal ICB (SRC IP/RTP)

27 94 00 04 0a 0a 24 16 27 95 00 04 00 00 00 01 \ ' Universal ICB (DST IP/RTP)

02 1e 13 00 03 00 13 00 02 00 06 00 06 00 02 00 01 00 0f 00 01 0b \ ' Router ICB

02 1e 07 00 01 01 db 00 01 02 \' Connection Mode TLV

The Resource Attribute Configure message below modifies the current connection to a one-way listen only connection:

00 1a 00 e3 00 00 ff \' Header

00 01 01 01 04 00 02 \' Router AIB

00 09 00 05 0d 03 00 01 00 \ ' Address Element TLV

01 db 00 01 01 \' Connection Mode TLV

The Resource Attribute Configure message below establishes a new one-way talk only connection:

00 2a 00 e3 00 00 ff \' Header

00 01 01 01 04 00 04 \' Router AIB

00 09 00 05 0d 03 00 01 00 \ ' Address Element TLV

27 94 00 04 0a 0a 24 16 \ ' Destination IP address TLV

27 95 00 04 00 00 00 01 \ ' Destination RTP port TLV

01 db 00 01 02 ' Connection Mode TLV

See Address Information Block.
See Information Control Block.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Real-Time Transport Protocol. Supports transport of real-time data like interactive voice and video over packet-switched networks.
The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.