0x0002 Remove IP Signaling Series 3 Card

Used in:
Matrix Configure message (0x7D)
IP Signaling Series 3 Card Configure message (0x0100)

Byte | Description
0, 1 | Tag 0x0002
2, 3 | Length 0x0002
4 | Value[0] IP Signaling Series 3 card ID to be removed, MSB: 0x00 Remove a specific IP Signaling Series 3 card 0xFF Remove every configured IP Signaling Series 3 cards
3 | Value[1] IP Signaling Series 3 card ID to be removed, LSB: 0x00-0x3F IP Signaling Series 3 card to be removed 0xFF Remove all configured IP Signaling Series 3 cards

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Most Significant Bit
Least Significant Bit