0x02D2 RAS RRQ Timer

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x2D2 RAS RRQ Timer Configure
2, 3 | Length 0x0002
4, 5 | Value[0, 1] 0x0064 (Default) All timer values are used in units of 10 ms each.

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
The Registration, Admission, and Status messages communicated between two H.323 entities for example between an Endpoint and a Gatekeeper.