0x02C6 Gateway URL ID

Important! You can deconfigure the Gateway URL ID by setting it to Null.

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x2C6 Gateway URL ID
2, 3 | Length Variable (maximim 512-byte ASCII character strings)
: | Value [n] 0-9, #, * Last character must be 0. Default is Null

A device that translates calls between an IP network and another network, typically the PSTN.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
American Standard Code for Information Interchange