0x275F Recognition Time
(Interworking Only)

Used in:
0x0033 NPDI Universal ICB

Byte | Description
0, 1 | Tag 0x275F
2, 3 | Length Variable
4 | Value[0] Signal Type Use values as defined in Pulsed Type (in Pulsed Signal TLV 0x275D) and Steady Signal Type (in Steady-Signal TLV 0x275E).
5 | Value[1] Duration Type Predefined description that is the actual value of the recognition time.

Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.