You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Resource Delete Indication 0x0129

Resource Delete Indication 0x0129

SwitchKit Name

Type

EXS API and SwitchKit API message

Description

Resource Delete Indication 0x0129

This message indicates that a resource has been deleted.

Conferencing

When a child conference has been deleted, this message uses the Child Conference ID AIB as well as the mandatory AIB Container TLV (0xE003).

Sent by

CSP

Related API Messages

Resource Create (0x0124)

Resource Modify (0x125)

Resource Delete (0x0126)

Resource Connect (0x127)

SwitchKit Code

C Structure

typedef struct {

UBYTE AddrInfo[30];

UBYTE DataType;

UBYTE TLVCount;

UBYTE Data[221];

} XL_ResourceDeleteIndication;

C++ Class

class XLC_ResourceDeleteIndication : public XLC_OutboundMessage {

public:

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

// Extended addressing functions

// Conference ID AIB functions

XBYTE getConferenceID() const;

void setConferenceID(XBYTE x);

XBYTE getParentConferenceID() const;

void setParentConferenceID(XBYTE x);

XBYTE getChildConferenceID() const;

void setChildConferenceID(XBYTE x);

void setChildConferenceID(XBYTE x);

UBYTE getDataType() const;

void setDataType(UBYTE x);

UBYTE getTLVCount() const ;

void setTLVCount(UBYTE x) ;

const UBYTE *getData() const ;

UBYTE *getData();

void setData(UBYTE *x) ;

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x00NN) | 1, 2 | Length (0x00NN)
3, 4 | Message Type (0x0129) | 3, 4 | Message Type (0x0129)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
8 | Address Information Block 0x45 Child Conference ID | 8 | Checksum
: | Data Type 0x00 (2-byte global TLVs) Mandatory TLVs 0xE003 AIB Container TLV - if indicating deletion of a child conference
: | Number of TLVs to Follow
: | :
: | Checksum

See Address Information Block.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
AIB. A standardized block that allows address data to be inserted in a standard way into API messages.