You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > EXS API Message Set

EXS API Message Set

(Access these messages from to the Contents in the left pane.)

Alarm 0x00B9

Alarm Cleared 0x00C1

Answer Supervision Mode Configure 0x00BB

ARP Cache Query 0x00FC

ARP Cache Report 0x00FB

Assign Logical Span ID 0x00A8

B Channel Configure 0x00C8

B Channel Query 0x00CA

Become Active 0x00A1

Busy Out 0x0018

Busy Out Flag Configure 0x00D3

Call Control Instructions Query 0x0087

Call Processing Event 0x002E

Call Progress Analysis Class Configure 0x00B3

Call Progress Analysis Configuration Query 0x008A

Call Progress Analysis Pattern Configure 0x00B2

Call Progress Analysis Result 0x0034

Card Population Query 0x0007

Card Status Query 0x0083

Card Status Report 0x00A6

CCS Redundancy Configure 0x005B

CCS Redundancy Query 0x006C

CCS Redundancy Report 0x0073

Channel Connection Status Query 0x0001

Channel Parameter Query 0x0080

Channel Release Request 0x0037

Channel Released 0x0049

Channel Released With Data 0x0069

Clear IP Signaling Series 3 Card 0x0108

Clear System Software 0x000C

Collect Digit String 0x00BC

Conference Create 0x004B

Conference Delete Request 0x004C

Conference Deleted 0x004D

Connect 0x0000

Connect One-Way Forced 0x0050

Connect One-Way To Conference 0x004F

Connect To Conference 0x004E

Connect Tone Pattern 0x002F

Connect Wait 0x0017

Connect With Data 0x0005

Connect With Pad 0x0003

CPC Detection 0x0047

Cross Connect Channel 0x001A

Cross Connect Span 0x001C

Cross Disconnect Channel 0x001B

Cross Disconnect Span 0x001D

D Channel Assign 0x00C4

D Channel De-assign 0x00C5

D Channel Facility List Configure 0x00C6

D Channel Facility List Query 0x00CB

Diagnostics Indication 0x0045

Disconnect Tone Pattern 0x001E

Distant End Release Mode 0x00B8

Download Begin BRecord 0x009B

Download Begin SRecord 0x00A2

Download BRecord 0x009C

Download Complete 0x00A4

Download SRecord 0x00A3

DS0 Status Change 0x0042

DS3 Configure/Query 0x000F

DSP Cache Modify 0x011A

DSP Service Cancel 0x00BE

DSP Service Request 0x00BD

DSP SIMM Configure 0x00C0

E1 Span Configure 0x00D8

E1 Span Query 0x00DB

EXNET Ring Configure 0x0074

EXS Node Configuration Query 0x007E

EXS Node Configure 0x007F

Fault Log Query 0x0086

Filter/Timer Configure 0x0012

Flash Timing Configure 0x0016

Generate Call Processing Event 0x00BA

Generic Card Configure 0x0122

Generic Card Query 0x0123

Generic Event Logger Configure/Query 0x003D

Generic Report 0x0046

Inpulsing Parameters Configure 0x0028

Inpulsing Parameters Query 0x0089

Inseize Control 0x002B

Inseize Instruction List Configure 0x0029

IP Address Configure 0x00E7

IP Address Query 0x00E6

IP Signaling Series 3 Card Configure 0x0100

IP Signaling Series 3 Card Host Poll 0x0104

IP Signaling Series 3 Card Query 0x0101

IP Signaling Series 3 Card Status Report 0x0105

IP Socket Configure 0x00F0

IP Socket Query 0x00F1

IP Socket Status Report 0x00F2

ISDN Interface Configure 0x0060

ISDN Query 0x0063

ISDN Terminal Configure 0x0062

J1 Span Configure 0x0019

Line Card Switchover 0x0024

Local End Release Mode Configure 0x0021

Loop Back Configure/Query 0x0091

Loop Timing Configure 0x004A

Matrix Configure 0x007D

Matrix Query 0x0097

Matrix Status Report 0x00E5

Multi-Host Configure 0x00E9

Node Status Query 0x006F

NGA Configure 0x0130

NGA Configure Query 0x0131

NGA Service Configure 0x0160

NGA Service Query 0x0161

NGA State Notify 0x0163

NGA State Notify 0x0163

Node Status Report 0x0070

Outpulse Digits 0x0020

Outseize Control 0x002C

Outseize Instruction List Configure 0x002A

Park Channel 0x00BF

PCM Encoding Format Configure 0x00D9

Play File Modify 0x011C

Play File Start 0x011B

Play File Stop 0x011D

Poll 0x00AB

Poll Interval Configure 0x009F

Poll Request 0x009E

PPL Assign 0x00D1

PPL Audit Configure 0x00DC

PPL Audit Query 0x00DD

PPL Configure 0x00D7

PPL Create 0x00D4

PPL Data Query 0x00DE

PPL Delete 0x00DA

PPL Event Indication 0x0043

PPL Event Request 0x0044

PPL Protocol Query 0x00DF

PPL Table Download 0x00D6

PPL Table Download Initiate 0x00D5

PPL Timer Configure 0x00CF

PPL Transmit Signal Configure 0x00D2

Product License Download 0x0079

Product License Query 0x007A

Receive Signaling Configure 0x0015

Record File Modify 0x011F

Record File Start 0x011E

Record File Stop 0x0120

Recorded Announcement Connect 0x0055

Recorded Announcement Delete 0x0054

Recorded Announcement Disconnect 0x0056

Recorded Announcement Download 0x0053

Recorded Announcement Download Initiate 0x0052

Recorded Announcement File System Convert 0x0118

Recorded Announcement File System Defragment 0x0103

Recorded Announcement File System Query 0x0102

Recorded Announcement File System Report 0x0119

Recorded Announcement Query 0x0057

Recorded Announcement Report 0x0058

Recorded Announcement Single Delete 0x0117

Release Channel 0x0008

Release Channel With Data 0x0036

Request For Service 0x0040

Request For Service With Data 0x002D

Reset Configuration 0x000B

Reset IP Signaling Series 3 Card 0x0107

Reset Matrix 0x009D

Resource Attribute Configure 0x00E3

Resource Attribute Query 0x00E4

Resource Connect 0x0127

Resource Create 0x0124

Resource Delete 0x0126

Resource Information Notify 0x0141

Resource Modify 0x0125

Resource Release Request 0x012D

Resource Release Indication 0x012E

Ring Status Query 0x0071

Ring Status Report 0x0072

Route Control 0x00E8

Service State Configure 0x000A

SNMP Configure 0x0092

Span Filter Configure 0x00CD

Span Filter Query 0x00CE

Span Status Query 0x0084

SS7 CIC Configure 0x006A

SS7 CIC Query 0x0067

SS7 CLLI Configure 0x00EA

SS7 CLLI Query 0x00EB

SS7 ISUP Message Format Configure 0x006B

SS7 ISUP Message Query 0x0068

SS7 SCCP/TCAP Configure 0x0077

SS7 SCCP/TCAP Query 0x0078

SS7 Signaling Link Configure 0x005E

SS7 Signaling Link Query 0x0065

SS7 Signaling Link Set Configure 0x005D

SS7 Signaling Link Set Query 0x0064

SS7 Signaling Route Configure 0x005F

SS7 Signaling Route Query 0x0066

SS7 Signaling Stack Configure 0x005C

SS7 Signaling Stack Query 0x006D

SS7 TUP Message Format Configure 0x008F

SS7 TUP Message Query 0x0090

Standby Line Card Configure 0x0023

Start Dial Configure 0x0013

Statistics Query 0x0121

Subrate Connection Management 0x000D

Synchronization Priority List Configure 0x0006

Synchronization Priority List Query 0x0081

System Configuration 0x00AF

System Configuration Query 0x00B4

System Log Query 0x0082

System Resource Usage Query 0x008E

T1 Span Configure 0x00A9

T1 Span Query 0x0085

Tag Configuration 0x00D0

TFTP Manage 0x003A

Time Set 0x00B5

Tone Configure 0x0031

Tone Query 0x005A

Transmit Cadence Pattern Configure 0x0030

Transmit Cadence Pattern Query 0x0059

Transmit Signaling Configure 0x0014

Trunk Type Configure 0x0011

V5 Configure 0x007B

V5 Configuration Query 0x007C

Version Request 0x0002

Virtual Card Configure 0x00E0

Virtual Span Control 0x00E2

VoIP Protocol Configure 0x00EE

VoIP Protocol Query 0x00EF

Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.
Bearer channel, 64Kbps (ISDN) The channel that carries the actual payload (as opposed to D-channels, which carry signaling data that helps route the payload).
Message delimiter (SS7 bit pattern - 01111110)
Setting up, monitoring, and tearing down calls.
See Common Channel Signaling.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Data channel. One of two fundamental components of an ISDN interface, it provides a path (16Kbps for BRI, 64Kbps for PRI) for carrying control signals and call data in a packet-switched mode.
Digital Signal Processor
A digital communications link - voice, data, and video at a 2.048 Mbps rate; 30B/2D or 31B/1D (ISDN); non-North American version of T1.
Excel's open architecture, proprietary, 1.3 Gbps fiber optic network using a packet-based protocol.
Quick depress and release of the phone plunger of a handset to signal the PBX or Centrex of instructions to follow (e.g., Call Transfer).
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
See Integrated Services Digital Network.
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.
Outgoing call setup during real-time call processing on a specific channel.
See Pulse Code Modulation.
See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
RFS. A Status Message indicating that some entity is requesting service from the Excel platform.
See Signaling System Number Seven.
See Circuit Identification Codes.
See Integrated Services Digital Network User Part.
See Transaction Capability Application Part.
Link that connects to the same node
Telephone User Part
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)
Pattern of tones and silence, such as a busy signal.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).