You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Reset IP Signaling Series 3 Card 0x0107

Reset IP Signaling Series 3 Card 0x0107

Type

EXS API message

Description

Reset IP Signaling Series 3 Card 0x0107

This message resets the IP Signaling Series 3 card before and/or after the IP Signaling Series 3 Card Interface is established. This message is sent directly to the IP Signaling Series 3 card and uses the extended logical node ID format.

You can also reset the IP Signaling Series 3 card using the Reset Configuration 0x000B message once the IP Signaling Series 3 Card Interface is established.

Sent by

Host

Example Message

The follow sample resets the IP Signaling Series 3 card when the IP Signaling Series 3 card ID or Matrix ID is not assigned.

00 11 01 07 00 00 fe 00 02 52 02 ff ff 53 04 00 20 ff ff

SwitchKit Code

C Structure

typedef struct {

UBYTE AddrInfo[4];

unsigned short ExpandedNode;

unsigned short ObjectType;

unsigned short ObjectInstanceID; ;

} XL_IPCallServerReset;

C++ Class

class XLC_IPCallServerReset: public XLC_OutboundMessage {

public:

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

unsigned short getExpandedNode() const;

void setExpandedNode(unsigned short x);

unsigned short getObjectType() const;

void setObjectType(unsigned short x)

unsigned short getObjectInstanceID const;

void setObjectInstanceID(unsigned short x)

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0x000B)
3, 4 | Message Type (0x0107) | 3, 4 | Message Type (0x0107)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Sequence Number (same as message)
7 | Extended Logical Node ID (0xFE) | 7 | Logical Node ID (0xFE)
8 : | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status MSB, LSB 0x0001
Number of AEs to follow
AE 0x48 Ring Communication Link 0x53 Object Type | 10-15 | AIB (same as message)
: | Checksum | 16-19 | AIB (same as message)
: | Checksum

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit