0x068B Input Gain Control

Use this TLV with the Channel AIB in the following messages to set the input gain, in decibels, for a conferee.

• Resource Create (0x0124)

• Resource Modify (0x0125)

• Resource Connect (0x0127)

Byte | Description
0, 1 | Tag: 0x068B Input Gain Control
2, 3 | Length: 0x0002
4-5 | Input Gain (in 1 db increments) Min -40 (0xFFD8) Max +10 (0x000A) Default 0 (0x0000)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Address Information Block.