0x002B MTP3 User Part Parameter

Used in:
PPL Event Request message
PPL Event Indication message

ICB Type | 0x03 (Extended Data)
ICB Subtype | 0x002B MTP3 User Part Parameter
ICB Length | Length of parameters, in bytes
Data[0] | Parameter 1 Type ID
Data[1] | Length of parameter 1data in bytes
Data[2] | Parameter 1 Value Variable size
: |
Data[:] | Parameter n Type ID
Data[:] | Length of parameter n data in bytes
Data[:] | Parameter n Value Variable size

PPL Parameters

ICB Type | 0x03 (Extended Data)
ICB ID | 0x0424
Data Length 2 bytes | 0x000D
Data[0-3] | DPC - Destination Point Code
Data[4-7] | OPC - Originating Point Code
Data[8-9] | CIC - Cirucuit ID Code
Data[10] | SI - Service Indicator
Data[11] | MP - Message Priority
Data[12] | NI - Network Indicator

ICB Type | 0x03 (Extended Data)
ICB ID | 0x0425
Data Length 2 bytes | 0x000C
Data[0-3] | DPC - Destination Point Code
Data[4-7] | OPC - Originating Point Code
Data[8] | SI - Service Indicator
Data[9] | MP - Message Priority
Data[10] | NI - Network Indicator
Data[11] | SLS - Signaling Link Set

ICB Type | 0x03 (Extended Data)
ICB ID | 0x0426
Data Length 2 bytes | Up to 0x010E
Data[0-1] | Length - Length of MSU Data
Data[4-n] | MSU Data - Length up to 0x010C

ICB Type | 0x03 (Extended Data)
ICB ID | 0x0427
Data Length 2 bytes | 0x0006
Data[0-3] | Affected DPC
Data[4] | Cause Value Value 0 - congestion level 0 Value 1 - congestion level 1 Value 2 - congestion level 2 Value 3 - congestion level 3 Value 4 - User Part Unavailable Value 5 - User Part Unequipped Value 6 - User Part Inaccessible Value 7 - Signaling Link Congestion level 0 Value 8 - Signaling Link Congestion level 1 Value 9: Signaling Link Congestion level 2 Value 10: Signaling Link Congestion level 3 Value 11: Signaling Link Congestion level 4
Data[5] | User Information Octet value

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.
Message Transfer Part level 3 - network level
Destination Point Code
A number that addresses a node in a SS7 network.
See Circuit Identification Codes.
Link that connects to the same node