L3P Call Control Configuration Bytes

Byte | Description | Values
--- | --- | ---
0x01 | Request for Service Format | * 0x01 = BCD Encoded 0x03 = Formatted ICB 0x04 = Exact Frame
0x02 | Send ALERTING Request to L3P | * 0x00 = Send 0x01 = Do Not Send
0x03 | Send DISCONNECT INDICATION to L5 | * 0x00 = Disable 0x01 = Enable
0x04 | Send ALERTING INDICATION to host | * 0x00 = Disable 0x01 = Enable
0x05 | Send PROGRESS to host | * 0x00 = Disable 0x01 = Enable
0x06 | Send CONNECT to host | * 0x00 = Disable 0x01 = Enable
0x07 | Send RELEASE (COMPLETE) to host | * 0x00 = Disable 0x01 = Enable
0x0C | Send Call Proceeding event to host upon receipt of CALL PROCEEDING indication from network | * 0x00 = Disable 0x01 = Enable
0x0E | Send Outseize ACK event to host upon receipt of CALL PROCEEDING indication from network | * 0x00 = Disable 0x01 = Enable
For Euro-ISDN only:
0x09 | Overlap Receive mode | * 0x00 = Disable (False) 0x01 = Enable (True)
0x0A | Overlap Receive Supported Digit Length | 10 digits
For Euro-ISDN and Austel only:
0x0B | Send Setup ACK and More Info event to host upon receipt of SETUP ACK indication from network | * 0x00 = Disable 0x01 = Enable
0x0D | Send Outseize ACK event to host upon receipt of SETUP ACK indication from network. | * 0x00 = Disable 0x01 = Enable

See Information Control Block.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.
Outgoing call setup during real-time call processing on a specific channel.
Positive acknowledgment to a message
See Integrated Services Digital Network.