PPL Event Indications Supported by MTP3 LSAC

Event ID | Event
--- | ---
0x0001 | Link Activation Failure
0x0002 | Signaling link failure. This is an existing PPL Event Indication to which Q.752 Parameters are added (unless operating under backward compatibility). A single ICB of type Q.752 Parameters is included with the following parameters: 0x0000 Timestamp 0x0001 Interval sequence number 0x001d Link failure reason code
0x0003 | Signaling link test failure. This is an existing PPL Event Indication to which Q.752 Parameters are added (unless operating under backward compatibility). A single ICB of type Q.752 Parameters is included with the following parameters: 0x0000 Timestamp 0x0001 Interval sequence number
0x0004 | Signaling link restoration. A single ICB of type Q.752 Parameters is included with the following parameters: 0x0000 Timestamp 0x0001 Interval sequence number

See Programmable Protocol Language.
See Information Control Block.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.