0x026A Use SIP Maximum Retransmissions Invite

Use this TLV to specify the maximum retransmissions for an INVITE request. The default value is 0x07.

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x026A
2, 3 | Length 0x0001
4 | Value[0] Maximum Number of Transmissions

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).