0x0119 Media Offer Stage

Use this TLV with the Alerting or Progress call processing event to ask for a media connection before the Answer message is sent.

Used in:
0x1E Generic PPL ICB in:
PPL Event Request message

Byte | Description
0, 1 | Tag 0x0119
2, 3 | Length 0x0002
4 | Value[0] 0x0000 - Do not offer media. 0x0001 - Offer media.

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.
See Programmable Protocol Language.
See Information Control Block.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.