0x03 Client Socket Register by Name

Used in:
IP Socket Configure message

Byte | Description
0 | Tag 0x03 Client Socket Register by Name
1 | Length 0x00D
2 | Value[0] 0x00 Module (0xFF = base board)
3 | Value[1] Socket ID
4-7 | Value[2-5] Local IP Address (4 bytes)
8 | Value[6] Local Port, MSB
9 | Value[7] Local Port, LSB
10 | Value[8] Remote Name Length
11 | Value[9] Remote Name[0]
12 | Value[10] Remote Name[1]
13 | Value[:] :
14 | Value[:] Remote Port, MSB
15 | Value[:] Remote Port, LSB

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
In SIP, an application program that sends SIP requests (See also Session Initiation Protocol). Clients may or may not interact directly with a person. Users agents and proxies contain clients (and servers).
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
Most Significant Bit
Least Significant Bit