0x293F NPDI SIP Authentication Timeout

Use this TLV to specify the timeout for authentication response.

Used in:
0x0033 NPDI Universal ICB in:
Route Control message
PPL Event Request message with Event IDs 0x0C

Byte | Description
0, 1 | Tag 0x293F
2, 3 | Length 0x01
4-n | Value[0-n] Timeout in seconds Minimum: 30 seconds Maximum: 255 seconds

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.
See Programmable Protocol Language.