You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Resource Attribute Configure 0x00E3

Resource Attribute Configure 0x00E3

SwitchKit Name

ResourceAttributeConfig

Type

EXS API and SwitchKit API message

Description

Resource Attribute Configure 0x00E3

Use this message to configure attributes on a VDAC-ONE card, IP Network Interface Series 2 card, or a VoIP module.

For VDAC-ONE cards, if a span/channel is active, this message waits until the call ends before updating the configuration.

For IP Network Interface Series 2 cards, you can change the payload size and type during the call.

Sent By

Host

SwitchKit Code

Configuration

ResourceAttributeConfig (

Node = integer,

Slot = integer,

DataType = integer,

TLVCount = integer,

Data = byte array);

C Structure

typedef struct {

UBYTE Slot;

UBYTE DataType;

UBYTE TLVCount;

UBYTE Data[221];

} XL_ResourceAttributeConfig;

C++ Class

class XLC_ResourceAttributeConfig : public XLC_OutboundMessage {

public:

UBYTE getSlot() const;

void setSlot(UBYTE x);

UBYTE getDataType() const;

void setDataType(UBYTE x);

UBYTE getTLVCount() const;

void setTLVCount(UBYTE x);

const UBYTE *getData() const;

UBYTE *getData();

void setData(UBYTE *x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0XFE) | 0 | Frame (0XFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0xNNNN)
3, 4 | Message Type (0x00E3) | 3, 4 | Message Type (0x00E3)
5 | Reserved | 5 | Reserved
6 | Sequence Number | 6 | Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
8 : | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status MSB, LSB
Number of AEs to follow | 10 | Checksum
AEs 0x01 Slot
: | Data Type 0x00 - TLVs
: | Number of TLV blocks to follow
: | Data (TLVs) 0x0009 Address Element TLV (Required if TLV 0x01E2 below is included in message.) 0x0100 RTP Payload Type (VDAC-ONE) 0x0100 RTP Payload Type (IPN Series 3) 0x0100 RTP Payload Type (IPN Series 2) 0x0101 RTP Payload Size (IPN Series 2) 0x0102 RTP Silence Suppression 0x0103 RTP Echo Cancellation 0x01C2 Minimum Jitter Buffer Delay 0x01C3 Maximum Jitter Buffer Delay (IPN-2 Card) 0x01C4 Adaptation Rate 0x01C5 Fax Type Enable 0x01C7 Fax/Modem Bypass Coder Type 0x01C8 Protocol Type 0x01D0 Gateway Mode 0x01D1 RTP Payload Redundancy 0x01D2 Fax Payload Redundancy 0x01D4 Type of Service 0x01D7 Default Domain Name 0x01DB Connection Mode 0x01DF UDP Source Port Validate 0x01E1 Fax Compatibility Mode 0x01E2 RFC 2833 Enable 0x01E5 VoIP Resource Profile Assign 0x01E6 Source T.38 Port 0x01E7 Destination T.38 Port 0x01E8 Source RTCP Port 0x01E9 Destination RTCP Port 0x01EB RTP Timer Timeout (VDAC-ONE) 0x01EB Initial Media Inactivity Timeout (IP Network Interface Series 2 Card) 0x01EC Media Inactivity Detection Timer 0x01F1 RFC 2833 Dynamic Payload Type 0x2794 Destination IP Address 0x2795 Destination RTP Port 0x27B0 RTP Payload Type
: | Checksum

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.