0x05E2 File Location

Use this TLV to specify the location of recorded voice files.

This TLV is mandatory for file IDs of 0x00100000 or higher in the Play File Start message, and in the Record File Start message.

It is also mandatory in the DSP Cache Modify message when the Action field is set to Copy.

Byte | Description
0, 1 | Tag 0x05E2 File Location
2, 3 | Length Variable
4, 5 | Value[0, 1] Primary Server ID
6, 7 | Value[2, 3] Secondary Server ID
8-N | Value[4-N] Filename, not including Mount name (must begin with / or \\ ) 128 characters maximum

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor