You are here: CSP Developer’s Guide: Common Channel Signaling > 5 TUP, BT IUP & SSUTR2 > BT IUP Configuration Examples

BT IUP Configuration Examples

Overview

This section provides configuration examples using the BT IUP protocol.

Examples

# Assign Logical Spans.

00 0D 00 a8 00 00 01 00 01 11 04 00 00 01 00

00 0D 00 a8 00 00 01 00 01 11 04 00 01 01 01

00 0D 00 a8 00 00 01 00 01 11 04 00 02 01 02

00 0D 00 a8 00 00 01 00 01 11 04 00 03 01 03

# Configure E1 Span format for HDB3, Clear Channel.

00 0F 00 d8 00 00 01 00 01 0C 02 00 00 09 00 F8 D0

00 0F 00 d8 00 00 01 00 01 0C 02 00 01 09 00 F8 D0

00 0F 00 d8 00 00 01 00 01 0C 02 00 02 09 00 F8 D0

00 0F 00 d8 00 00 01 00 01 0C 02 00 03 09 00 F8 D0

# Download SS7 License here.

# Configure CCS Redundancy.

# Primary Slot 8, Secondary Slot 9.

00 0E 00 5B 00 00 01 00 02 01 01 02 01 01 03 00

# Configure the SS7 Stack.

# Stack ID 0, OPC 0x00000123 0-36-3

# 4 Modules

# MTP/ITU, L3P/ITU, L3P-TUP/IUP, TUP/IUP

00 18 00 5c 00 00 01 00 01 21 02 08 00 00 00 01 23 04 01 01 03 01 04 02 05 02

# Configure the SS7 Linkset

# Linkset 0, APC 0x00000987 1-48-7

00 0F 00 5D 00 00 01 00 01 1E 02 00 00 00 00 00 09 87

# Configure the SS7 Link

# Linkset 0, Link ID 0, SLC 0, Data rate 64k

# Span 0, Channel 30

00 21 00 5E 00 00 01 00 02 1F 03 00 00 00 0d 03 00 00 1e 00 00 00

# Configure the SS7 Route

# Linkset 0, Destination 0, Route 0, DPC 0x00000987 1-48-7

00 13 00 5F 00 00 01 00 01 20 05 00 00 00 00 00 00 00 09 87 00 00 00 FF FF

$cic: (0100)

$log_span_id: (00 02)

$channel: (00)

$nbr_cics: (01)

$call_ctrl_user_part: (01) ' TUP

00 17 00 6A 00 00 01 00 01 14 07 00 00 00 $log_span_id $channel $nbr_cics $dest_point_code $call_ctrl_user_part

# SS7 CIC Configure

# These are done span by span. CIC numbering must match on each side

# Setup CICs on span w/ Link of SLC=0

00 15 00 6a 00 00 01 00 01 14 07 00 00 00 00 00 00 0f 00 00 09 87 00

00 15 00 6a 00 00 01 00 01 14 07 00 00 10 00 00 0f 0f 00 00 09 87 00

'Setup CICs on second span

00 15 00 6a 00 00 01 00 01 14 07 01 00 20 00 01 00 1f 00 00 09 87 00

'Setup CICs on third span

00 15 00 6a 00 00 01 00 01 14 07 00 00 40 00 02 00 1f 00 00 09 87 00

'Setup CICs on fourth span

00 15 00 6a 00 00 01 00 01 14 07 01 00 60 00 03 00 1f 00 00 09 87 00

# Bring Span In Service

00 0D 00 0A 00 00 01 00 01 0C 02 00 00 F0 00

00 0D 00 0A 00 00 01 00 01 0C 02 00 01 F0 00

00 0D 00 0A 00 00 01 00 01 0C 02 00 02 F0 00

00 0D 00 0A 00 00 01 00 01 0C 02 00 03 F0 00

# Bring SS7 Link In Service

00 0D 00 0a 00 00 01 00 01 09 02 00 00 F0 00

# Bring SS7 CIC's In Service

00 13 00 0a 00 00 01 01 02 0D 03 00 00 00 0D 03 00 00 0f f0 00

00 13 00 0a 00 00 01 01 02 0D 03 00 00 10 0D 03 00 00 1d f0 00

00 13 00 0a 00 00 01 01 02 0D 03 00 01 00 0D 03 00 01 1e f0 00

00 13 00 0a 00 00 01 01 02 0D 03 00 02 00 0D 03 00 02 1e f0 00

00 13 00 0a 00 00 01 01 02 0D 03 00 03 00 0D 03 00 03 1e f0 00

A digital communications link - voice, data, and video at a 2.048 Mbps rate; 30B/2D or 31B/1D (ISDN); non-North American version of T1.
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.
Signaling technique where the full channel bandwidth is used for data transmission, while the framing and control bits (signaling) use a separate channel. No control or signaling is performed on this path. See B8ZS and ZBTSI.
See Signaling System Number Seven.
See Common Channel Signaling.
See Message Transfer Part.
International Telecommunications Union (UN)
Telephone User Part
Destination Point Code
See Circuit Identification Codes.