You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Card Status Query 0x0083

Card Status Query 0x0083

SwitchKit Name

CardStatusQuery

Type

EXS API and SwitchKit API message

Description

Card Status Query 0x0083

Use this message to get a report on a specified card type.

The host can also send this message to the active or standby CSP Matrix Series 3 Card.

Sent by

Host

SwitchKit Code

C Structure

typedef struct {

} XL_CardStatusQuery;

C Structure Response

typedef struct {

unsigned short Status;

UBYTE AddrInfo[30];

UBYTE CardType;

UBYTE CardStatus;

UBYTE ConfTestRslts;

UBYTE ArtRevision;

UBYTE FunctRevision;

UBYTE ROMMajorRevision;

UBYTE ROMMinorRevision;

UBYTE RAMMajorRevision;

UBYTE RAMMinorRevision;

unsigned short SerialNumber;

unsigned short RAMSize;

UBYTE CardSpecifics[384];

UBYTE HardwareConfig[16];

UBYTE CardID;

UBYTE RAMBuildNum;

unsigned short ConfigTag;

UBYTE LineCardSpeed;

UBYTE SoftwareResetReason;

} XL_CardStatusQueryAck;

C++ Class

class XLC_CardStatusQuery : public XLC_OutboundMessage {

public:

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

// Extended addressing functions

// Slot AIB functions

UBYTE getSlot() const;

void setSlot(UBYTE x);

// Module AIB functions

UBYTE getModule() const;

void setModule(UBYTE x);

};

C++ Class Response

class XLC_CardStatusQueryAck : public XLC_AcknowledgeMessage {

public:

unsigned short getStatus() const;

void setStatus(unsigned short x);

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

UBYTE getSlot() const;

void setSlot(UBYTE x);

UBYTE getModule() const;

void setModule(UBYTE x);

UBYTE getCardType() const;

void setCardType(UBYTE x);

UBYTE getCardStatus() const;

void setCardStatus(UBYTE x);

UBYTE getConfTestRslts() const;

void setConfTestRslts(UBYTE x);

UBYTE getArtRevision() const;

void setArtRevision(UBYTE x);

UBYTE getFunctRevision() const;

void setFunctRevision(UBYTE x);

UBYTE getROMMajorRevision() const;

void setROMMajorRevision(UBYTE x);

UBYTE getROMMinorRevision() const;

void setROMMinorRevision(UBYTE x);

UBYTE getRAMMajorRevision() const;

void setRAMMajorRevision(UBYTE x);

UBYTE getRAMMinorRevision() const;

void setRAMMinorRevision(UBYTE x);

;}

Overview of message

The following table provides an overview of this message. The table following it, provides the detail for each byte.

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0xNNNN)
3, 4 | Message Type (0x0083) | 3, 4 | Message Type (0x0083)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB (starting with byte 0) | 8, 9 | Status MSB, LSB
: | :
: | Checksum | 10 | AIB
| Response continued below.
: | Card Type
: | Card Status
: | Confidence Test Results
: | PC Artwork Revision
: | Functional Revision
: | ROM Major Revision
: | ROM Minor Revision
: | RAM Major Revision
: | RAM Minor Revision
2 bytes | Serial Number MSB, LSB
2 bytes | RAM Size MSB, LSB
: | Card Information (Field length varies)
16 bytes | Hardware Configuration (16 bytes)
: | Card ID
: | RAM Build Number
2 bytes | Configuration Tag MSB, LSB
: | CPU Speed
: | Software Reset Reason
: | Checksum

EXS API Hex Format - Detailed

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0xNNNN)
3, 4 | Message Type (0x0083) | 3, 4 | Message Type (0x0083)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status MSB, LSB
: | AIB Same AIB sent in message
Number of AEs to follow
AEs 0x01 Slot or 0x42 VoIP Module
: | Checksum
| Response continued below.
: | Card Type
| 0x00 8-Span ST1LC 0x0 1 4-Span ST1LC 0x03 MFDSP 0x0A SS7 0x0B SE1LC 4-Span 0x0C SE1LC 8-Span 0x0E SJ1LC 4-Span 0x13 ISDN PRI 0x14 DASS 2 0x15 DSP-ONE 0x16 T-ONE 8-Span 0x17 E-ONE 8-Span 0x18 T-ONE 16-Span 0x19 E-ONE 16-Span 0x1D J-ONE 8-Span 0x1E J-ONE 16-Span 0x1F DS3 0x33 Subrate Controller
| 0x42 EXNET Connect PCI H.100 0x50 SS7 PQ 0x54 EXNET-ONE 0x60 VDAC ONE 0x61 VDAC VoIP Module 0x65 IP Network Interface Series 2 0x6B DSP Series 2 0x6D IP Network Interface Series 2 VoIP Module 0x6E Mindspeed VoIP Module 0x71 SS7 Series 3 0x72 CSP 2000 Matrix I/O 0x73 CSP 2000 Matrix 2000 0x75 CSP 2000 Matrix 1000 0x76 ISDN Series 3 0x79 IP Signaling Series 3 0x80 Virtual 32 Span VDAC-ONE or IP Media Series 2 0x90 DSP Series 2 Plus 0x91 IP Network Interface Series 3 0x92 Multi-Function Media I/O Plus 0xAA Ilegal I/O 0xCA Multi-Function Media I/O 0xCC DS3 Standby I/O 0xCF VDAC I/O 0xD2 Virtual T1 16-span 0xD5 Virtual E1/J1 16-Span 0xD8 CCS I/O Series 3 0xDB J-ONE Redundant I/O 0xDC J-ONE Standby I/O 0xDD DS3 Redundant I/O 0xDF CCS I/O
| 0xE0 E-ONE 75 Ohm Redundant I/O 0xE1 T-ONE 100 Ohm Redundant I/O 0xE2 E-ONE 120 Ohm Redundant I/O 0xE3 E-ONE 75 Ohm Standby I/O 0xE4 T-ONE 100 Ohm Standby I/O 0xE5 E-ONE 120 Ohm Standby I/O 0xE8 SS7 Multi-Protocol I/O
| 0xF0 Power Supply Card 0xF3 Matrix I/O 0xF5 EXNET Ring I/O 0xF6 Rear Fan Tray 0xF7 SS7 Redundant I/O
| 0xF8 Front Fan Tray 0xF9 ISDN Redundant I/O 0xFA Midplane 0xFE Dead Card: All subsequent data fields do not apply and all other bytes in the message should be ignored. 0xFF Empty Slot: All subsequent data fields do not apply.
: | Card Status This field is a bit mask that applies to the following cards: CSP Matrix Series 3 Card, T-ONE, E-ONE, J-ONE, DS3, EXNET-ONE, SS7-PQ, SS7 Series 3, DSP-ONE, MFDSP, DSP Series 2, DSP Series 2 Plus, ISDN PRI, ISDN Series 3, ST1LC, SE1LC, SJ1LC, VDAC-ONE, IP Network Interface Series 2/3, IP Signaling Series 3 Bit 0–1 Reset Reason 0 Dialogic use only 1 Power-up 2 Dialogic use only 3 Reset button pushed 2–3 Card State 0 In service 1 The CSP has taken the card out of service 2 The host has taken the card out of service 3 The host has put the card in a standby state 4 Invalid battery-backed configuration data. The host must reconfigure the card 5 Faults are logged Faults may be obtained using a Fault Log Query message. Obtain a Fault Log and report it to Dialogic Technical Support as soon as possible. 6 Failed confidence tests. Information about the confidence test which failed is in the "Confidence Test Results" field. 7 General hardware failure The card is off-line and must be serviced. See the Hardware Configuration Field for additional information on the ISDN PRI card.
| Fan Tray Bit 0 Reserved 1 Fan 6 failed 2 Fan 5 failed 3 Fan 4 failed 4 Fan 3 failed 5 Fan 2 failed 6 Fan 1 failed 7 General hardware failure. The card is off-line and must be serviced. Power Supply Card Bit 0 Module 3 failed 1 Module 3 in tolerance 2 Module 2 failed 3 Module 2 in tolerance 4 Module 1 failed 5 Module 1 in tolerance 6 Out of Tolerance 7 General hardware failure. The card is off-line and must be serviced. DS3, T1, E1, and J1 Redundant and Standby I/O Cards Bit 0–5 Reserved 6 Output Enabled 7 Relays Enabled (0=Normal, 1=Switchover) Matrix I/O Card Bit 0 Interface B link state: 0=Down, 1=Up 1 Interface A link state: 0=Down, 1=Up 2 The active Ethernet Interface: 0=Interface A. 1=Interface B
: | Confidence Test Results This field is bit-defined. It applies to the CSP Matrix Series 3 Card cards and line cards. Bit 0–5 Reserved 6 Bit set indicates RAM test failure 7 Bit set indicates ROM checksum failure
: | PC Artwork Revision An ASCII character in the range "A" to "Z" (0x41–0x5B) that indicates the revision level of the card’s Printed Circuit Artwork.
: | Functional Revision The card’s functional revision level
: | ROM Major Revision The major revision level of the firmware running on the card.
: | ROM Minor Revision The minor revision level of the firmware running on the card.
: | RAM Major Revision The major revision level of the system software running on the card.
: | RAM Minor Revision The minor revision level of the system software running on the card.
: | Serial Number MSB, LSB
This two-byte field indicates the serial number of the card.
: | RAM Size MSB, LSB This two-byte field indicates the amount of RAM on the card, in 1K increments. For the VDAC VoIP Card and VDAC VoIP Module, RAM is measured in 1 MB increments.
: | Card Information (Field length varies)
| The card information, including the length of the field, varies per card type. The system uses the value 0x00 for fields that do not apply to the card or for all fields, if there is no card information. IP Signaling Series 3 Card No card specific or hardware specific information is sent for this card. T-ONE, E-ONE, J-ONE, DS3, ST1LC, SE1LC, VDAC-ONE, IP Network Interface Series 2/3, and SS7 Multi- Protocol cards. The card information for these cards indicates the logical spans assigned to the card. The logical spans are indicated in the Logical Span AIB (0x0C) as shown below. The CSP uses the value 0xFF to indicate that no span has been assigned. An AIB for a 4-span line card has four address elements and the value 0x00 for the remaining bytes. An AIB for an 8-span line card has eight address elements and the value 0x00 for the remaining bytes. Data[0] Address Method (0x00, Single Entity) Data[1] Number of Address Elements ( equal to number of spans) Address Element 1: Span 0 Data[2] Address Type (0x0C, Logical Span) Data[3] Data Length (0x02) Data[4] Logical Span ID, MSB Data[5] Logical Span ID, LSB Address Element N: Span N Data[...] Address Type (0x0C, Logical Span) Data[...] Data Length (0x02) Data[...] Logical Span ID, MSB Data[...] Logical Span ID, LSB
| MFDSP and DSP-ONE Cards The card information for the DSP-ONE cards indicates the function types for DSPs on all SIMMs on the card. NOTE: For more information on function types, refer to the DSP SIMM Configure (0xC0) message. Byte Function Type Data[0] SIMM 0/DSP 0 Data[1] SIMM 0/DSP 1 Data[2] SIMM 0/DSP 2 Data[3] SIMM 0/DSP 3 Data[4] SIMM 1/DSP 0 Data[5] SIMM 1/DSP 1 Data[6] SIMM 1/DSP 2 Data[7] SIMM 1/DSP 3 Data[8] SIMM 2/DSP 0 Data[9] SIMM 2/DSP 1 Data[10] SIMM 2/DSP 2 Data[11] SIMM 2/DSP 3 Data[12] SIMM 3/DSP 0 Data[13] SIMM 3/DSP 1 Data[14] SIMM 3/DSP 2 Data[15] SIMM 3/DSP 3 Data[16–33] Reserved
| DSP Series 2 and DSP Series 2 Plus Cards The card information for the DSP Series 2 and DSP Series 2 Plus cards indicates the function types for all DSPs on all Modules on the card, because each DSP can do multiple configurations. Byte Function Type Data[0] Module 0 / DSP 0 / RCV 0 Data[1] Module 0 / DSP 0 / TXMT 0 Data[2] Module 0 / DSP 0 / RCV 1 Data[3] Module 0 / DSP 0 / TXMT 1 Data[4] Module 0 / DSP 1 / RCV 0 Data[5] Module 0 / DSP 1 / TXMT 0 Data[6] Module 0 / DSP 1 / RCV 1 Data[7] Module 0 / DSP 1 / TXMT 1 Data[8] Module 0 / DSP 2 / RCV 0 Data[9] Module 0 / DSP 2 / TXMT 0 Data[10] Module 0 / DSP 2 / RCV 1 Data[11] Module 0 / DSP 2 / TXMT 1 Data[12] Module 0 / DSP 3 / RCV 0 Data[13] Module 0 / DSP 3 / TXMT 0 Data[14] Module 0 / DSP 3 / RCV 1 Data[15] Module 0 / DSP 3 / TXMT 1 Data[16] Module 1 / DSP 0 / RCV 0 Data[17] Module 1 / DSP 0 / TXMT 0 Data[18] Module 1 / DSP 0 / RCV 1 Data[19] Module 1 / DSP 0 / TXMT 1 Data[20] Module 1 / DSP 1 / RCV 0 Data[21] Module 1 / DSP 1 / TXMT 0 Data[22] Module 1 / DSP 1 / RCV 1 Data[23] Module 1 / DSP 1 / TXMT 1 Data[24] Module 1 / DSP 2 / RCV 0 Data[25] Module 1 / DSP 2 / TXMT 0 Data[26] Module 1 / DSP 2 / RCV 1 Data[27] Module 1 / DSP 2 / TXMT 1 Data[28] Module 1 / DSP 3 / RCV 0 Data[29] Module 1 / DSP 3 / TXMT 0 Data[30] Module 1 / DSP 3 / RCV 1 Data[31] Module 1 / DSP 3 / TXMT 1 Data[32] Reserved Data[33] Reserved
| EXNET-ONE This card generates no special information for this field. All bytes are 0x00. SS7 Card Data[0] Maximum Configurable Links for card Data[1] Slot Number of Active SS7 Card (see Note) Data[2] Slot Number of Secondary SS7 Card in Redundant Pair (see Note) Data[3] Stack ID Data[4] Stack ID Data[5] Stack ID Data[6] Stack ID Data[7–15] Reserved NOTE: Do not try to determine the redundancy status from bytes Data[1] and Data[2]. To determine the redundancy status, use the CCS Redundancy Query message.
| Redundant I/O and Standby I/O A Slot AIB indicates the slot number of the other I/O (Standby I/O or Redundant I/O) involved in a switchover.
| PCI H.100 Card The card information fields depend upon on H.100 bus clock speed and the number of spans per channel. 4MHz and 24 channels per span display 21 span entries 4MHz and 32 channels per span display 16 span entries 8MHz and 24 channels per span display 80 span entries 8MHz and 32 channels per span display 64 span entries
: | Hardware Configuration (16 bytes) This 16-byte field describes the hardware configuration of the card specified. This field applies to only the cards described below. DS3 Cards Data[0] Number of SS7 Spans Supported: 0x18 24 Spans 0x1C 28 Spans Data[1] DS3 Offset Framer Status Bit 0 - DS3 Offset 0 Framer Status 0 - Out of Service 1 - In Service (default) Bit [1-7] Reserved Data [2-13] Reserved Data[14] Hardware Switch 1 Settings (also refer to the Hardware Product Descriptions) (the right-most bit is dip 1) Data[15] Total Available Spans
| ST1LC and SE1LC cards Data[0] Informs the host of primary and secondary loop timing clock sources configured on the card. Bits 0-2 If secondary loop timing is enabled, this field contains the offset of the span for which it is enabled. Bit 3 Secondary Loop timing 0 Disabled 1 Enabled Bit 4-6 If primary loop timing is enabled, this field contains the offset of the span for which it is enabled. Bit 7 Primary Loop timing 0 Disabled 1 Enabled Data[1-15] Reserved T-ONE, E-ONE, J-ONE cards Data 0–3 Informs the host of primary and secondary loop timing clock sources configured on the card Data[0] Primary Loop Timing 0 Not Enabled 1 Enabled Data[1] If Primary Loop Timing is enabled, this field contains the span offset of the span for which it is enabled. Data[2] Secondary Loop Timing 0 Not enabled 1 Enabled Data[3] If Secondary Loop Timing is enabled, this field contains the span offset of the span for which it is enabled. Data[4–13] Reserved Data[14] Hardware Switch 1 Settings (also refer to the Hardware Product Descriptions) (the right-most bit is dip 1) Data[15] Total Available Spans
| MFDSP and DSP-ONE Card This field informs the host of the number and types of DSP SIMMs installed on the card. Data[0] Number of DSP SIMMs installed on the card Data[1] Reserved Data[2] SIMM 0 Type 0x00 C31 SIMM 0x01 VRA SIMM 0x03 No SIMM installed Data[3] SIMM 1 Type 0x00 C31 SIMM 0x01 VRA SIMM 0x03 No SIMM installed Data[4] SIMM 2 Type 0x00 C31 SIMM 0x01 VRA SIMM 0x03 No SIMM installed Data[5] SIMM 3 Type 0x00 C31 SIMM 0x01 VRA SIMM 0x03 No SIMM installed
| Data 6-9: SIMM State 0 - SIMM State 3 0x00 In Service 0x01 Out of Service (or No SIMM Installed) Data[6] SIMM 0 State Data[7] SIMM 1 State Data[8] SIMM 2 State Data[9] SIMM 3 State Data[10–15] Reserved
| DSP Series 2 and DSP Series 2 Plus Cards This field informs the host of the number and types of DSP Modules installed on the card. Data[0] Number of Modules installed on the card Data[1] Reserved Data[2] Module 0 Type 0x6C DSP 2 Module 0x03 No Module installed Data[3] Module 1 Type 0x6C DSP 2 Module 0x03 No Module installed Data[4, 5] Reserved Data 6-13: DSP Chip States 0x00 In Service 0x01 Out of Service (or No Module Installed) Data[6] Module 0 / Chip 0 State Data[7] Module 0 / Chip 1 State Data[8] Module 0 / Chip 2 State Data[9] Module 0 / Chip 3 State Data[10] Module 1 / Chip 0 State Data[11] Module 1 / Chip 1 State Data[12] Module 1 / Chip 2 State Data[13] Module 1 / Chip 3 State Data[14-15] Reserved
| ISDN PRI Card Data[0] Munich Chip Count Data[1-15] Reserved
| EXNET-ONE card Data[0–3] Informs host of primary and secondary loop timing clock sources configured from ring timing on the card. For EXNET-ONE cards configured as a Single Ring Redundancy Standby, the Loop Timing fields are always disabled. Data[0] Primary Loop Timing 0x00 Not Enabled 0x01 Enabled Data[1] Reserved Data[2] Secondary Loop Timing 0x00 Not Enabled 0x01 Enabled Data[3] Reserved SS7 cards The system does not report hardware configuration information for these cards. All bytes are 0x00.
| SS7 Multi-Protocol I/O card Data[0] Channel 0 Data Rate 0x00 64 Kbps 0x01 56 Kbps, for non-V.35 applications 0x80 V.35, 56 Kbps 0x81 48 Kbps, for non-V.35 applications 0xC0 V.35, 48 Kbps Data[1] Channel 0 Electrical Interface 0x00 No Timing 0x01 V.35, DTE 0x02 V.35, DCE Data[2] Channel 1 Data Rate (same possibilities as Channel 0, above) Data[3] Channel 1 Electrical Interface (same possibilities as Channel 0, above) Data[4] Channel 2 Data Rate (same possibilities as Channel 0, above) Data[5] Channel 2 Electrical Interface (same possibilities as Channel 0, above) Data[6] Channel 3 Data Rate (same possibilities as Channel 0, above) Data[7] Channel 3 Electrical Interface (same possibilities as Channel 0, above) VDAC-ONE card Data[0] Number of VoIP Modules (1 - 4) Data[1] Number of channels supported (MSB) Data[2] Number of channels supported (LSB) Data[3] Installed VoIP Modules (Bit Field): Bit 0 VoIP Module 0 (0 = not installed, 1 = installed) Bit 1 VoIP Module 1 (0 = not installed, 1 = installed) Bit 2 VoIP Module 2 (0 = not installed, 1 = installed) Bit 3 VoIP Module 3 (0 = not installed, 1 = installed) Data[4] Module 0 state (0x05=ready, other values=not ready) Data[5] Module 1 state (0x05=ready, other values=not ready) Data[6] Module 2 state (0x05=ready, other values=not ready) Data[7] Module 2 state (0x05=ready, other values=not ready) Data[8] Port Consumption Mode 1 Reserved 2 Port-Consuming Data[9-15] Reserved (should be zero)
| VDAC VoIP Module Data[0] Total number of channels supported on the module Data[1] Number of channels supported for DSP 0 Data[2] Number of channels supported for DSP 1 Data[3] Number of channels supported for DSP 2 Data[4] Number of channels supported for DSP 3 Data[5] Number of channels supported for DSP 4 Data[6] Number of channels supported for DSP 5 Data[7] Number of channels supported for DSP 6 Data[8] Number of channels supported for DSP 7 Data[9-15] Reserved (should be zero) IP Network Interface Series 2 card Data[0] Number of VoIP Modules (0 - 2) Data[1] Number of channels supported (MSB) Data[2] Number of channels supported (LSB) Data[3] Installed VoIP Modules (Bit Field): Bit 0 VoIP Module 0 (0 = not installed, 1 = installed) Bit 1 VoIP Module 1 (0 = not installed, 1 = installed) Bit 2 VoIP Module 2 (0 = not installed, 1 = installed) Note that for Data 4 - 6 each module can be in one of the following states: 0x02 - Not Present, 0x05 - In Service, 0x06 - Out of Service, and 0x08 - Failed Data[4] Module 0 State Data[5] Module 1 State Data[6] Module 2 State Note that for Data 7 - 9 each module can be to one of the following IP resource profiles: 0x01 - G.711 Only (16 spans per module) 0x02 - G.711 + G.723.1 + G.729 + T.38 (8 spans per module) 0x0F - Not applicable (For example, module is not present) Data[7] Module 0 Profile Data[8] Module 1 Profile Data[9] Module 2 Profile Data[10] Port Consumption Mode 1 = Non Port-Consuming 2 = Port-Consuming Data[11-14] Refer to IPN-3 card Data[15] Reserved (Set to 0)
| IP Network Interface Series 2 Card Module Data[0] Total number of channels supported for the module (MSB) Data[1] Total number of channels supported for the module (LSB) Data[2] Module State Data[3] Module Profile Data[4] Bitmap of installed DSPs on a VoIP module (1 - Installed) Data[5] Bitmap of available DSPs on a VoIP module (1 - available) Data[6] Number of channels per available DSP Data[7] MII Bridge FPGA Version Data[8 - 15] Reserved (Set to 0) IP Network Interface Series 3 Card Data[0] Number of VoIP Modules (0 - 1) Data[1] Number of channels supported (MSB) Data[2] Number of channels supported (LSB) Data[3] Installed VoIP Modules (Bit Field): Bit 0 VoIP Module 0 (0 = not installed, 1 = installed) Bit 1 VoIP Module 1 (0 = not installed, 1 = installed) Data[4] Module 0 State Data[5] Module 1 State Note that for Data 4 - 5 each module can be in one of the following states: 0x02 - Not Present, 0x05 - In Service, 0x06 - Out of Service, and 0x08 - Failed Data[6] Module 0 Profile Data[7] Module 1 Profile Note that for Data 6-7 each module can be to one of the following IP resource profiles: 0x04 - G.711 Only (16 spans per module) 0x05 - LBR + T.38 (8 spans per module) 0x0F - Not applicable (For example, module is not present) Data[8] Port Consumption Mode 1 = Non Port-Consuming 2 = Port-Consuming Data[9] Main board dip switch settings (bit mask) (first value is default). Refer to the CSP Hardware Product Description for the IPN-3 card.
| Data[10] Port 0 Info (CTRL 0) Bit 0 Ethernet Link Status 0 = Ethernet link down 1 = Ethernet link up Bit 1 Duplex Type 0 = Half Duplex 1 = Full Duplex Bit 2-3 Speed 0 0 = 10Mbps 0 1 = 100Mbps 1 0 = 1000Mbps Bits [4-7] Reserved (should be zero) IPN-3 card Data[11] Port 1 Info (CTRL 1) Bit 0 Ethernet Link Status 0 = Ethernet link down 1 = Ethernet link up Bit 1 Duplex Type 0 = Half Duplex 1 = Full Duplex Data[12] Port 2 Info (DATA 0) Bit 0 Ethernet Link Status 0 = Ethernet link down 1 = Ethernet link up Bit 1 Duplex Type 0 = Half Duplex 1 = Full Duplex Bit 2-3 Speed 0 0 = 10Mbps 0 1 = 100Mbps 1 0 = 1000Mbps Bits [4-7] Reserved (should be zero) Data[13] Port 3 Info (DATA 1) Bit 0 Ethernet Link Status 0 = Ethernet link down 1 = Ethernet link up Bit 1 Duplex Type 0 = Half Duplex 1 = Full Duplex Bit 2-3 Speed 0 0 = 10Mbps 0 1 = 100Mbps 1 0 = 1000Mbps Bits [4-7] Reserved (should be zero) Bit 0 Ethernet Link Status 0 = Ethernet link down 1 = Ethernet link up Bit 1 Duplex Type 0 = Half Duplex 1 = Full Duplex
| Bit 2-3 Speed 0 0 = 10Mbps 0 1 = 100Mbps 1 0 = 1000Mbps Bits [4-7] Reserved (should be zero) Data[14] Port 4 Info (DATA 2) Bit 0 Ethernet Link Status 0 = Ethernet link down 1 = Ethernet link up Bit 1 Duplex Type 0 = Half Duplex 1 = Full Duplex Bit 2-3 Speed 0 0 = 10Mbps 0 1 = 100Mbps 1 0 = 1000Mbps Bits [4-7] Reserved (should be zero) Data[15] Port 5 Info (DATA 3) Bit 0 Ethernet Link Status 0 = Ethernet link down 1 = Ethernet link up Bit 1 Duplex Type 0 = Half Duplex 1 = Full Duplex Bit 2-3 Speed 0 0 = 10Mbps 0 1 = 100Mbps 1 0 = 1000Mbps Bits [4-7] Reserved (should be zero) IP Network Interface Series 3 Card Module Data[0] Total number of channels supported for the module (MSB) Data[1] Total number of channels supported for the module (LSB) Data[2] Module State Data[3] Module Profile Data[4] Bitmap of installed DSPs on a VoIP module (1 - Installed) Data[5] Bitmap of available DSPs on a VoIP module (1 - available) Data[6] Number of channels per available DSP
: | MAC Addresses Data[0,1] Reserved Data[2-5] 1C 03 35 51 MAC Address for Ethernet Port A Data[6-9] 1C 03 35 51 MAC Address for Ethernet Port A Data[10-17] Reserved
: | Card ID This field contains additional information about identification for the card.
: | RAM Build Number This field indicates the application build number of the system software.
: | Configuration Tag MSB, LSB The configuration tag number assigned by the Tag Configuration message.
: | CPU Speed This field applies to cards other than CSP Matrix Series 3 Cards. If the system is reporting on a CSP Matrix Series 3 Card, this field is not included in the report. 0x00 16 Mhz 0x01 16 Mhz 0x02 20 Mhz 0x03 20 Mhz 0x04 25 Mhz 0x05 50 Mhz 0x08 66 Mhz 0x09 83 Mhz 0x0A 100 Mhz
: | Software Reset Reason This field is reserved for Dialogic use only (it applies to cards other than matrix cards. For example, if the system is reporting on a CSP Matrix Series 3 Card, this field is not included in the report).
: | Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
See Address Information Block.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
Most Significant Bit
Least Significant Bit
Read Only Memory
Random Access Memory
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.
See Signaling System Number Seven.
See Integrated Services Digital Network.
Digital Signal Processor
Excel's open architecture, proprietary, 1.3 Gbps fiber optic network using a packet-based protocol.
Peripheral Component Interconnect
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)
A digital communications link - voice, data, and video at a 2.048 Mbps rate; 30B/2D or 31B/1D (ISDN); non-North American version of T1.
See Common Channel Signaling.
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.
American Standard Code for Information Interchange
The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.
Connection used for the transmission of high-speed data.
Data Terminal Equipment. According to the RS-232-C standard, DTE devices are typically personal computers or data terminals. See DCE.
Data Communications Equipment. According to the RS-232-C standard, DCE devices are typically modems or printers. See DTE.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."