You are here: CSP Hardware Product Descriptions > 4 Common Channel Signaling Cards > Dialogic® CCS I/O Series 3 Card - EXS7IO1300/EXS7IO1300R

Dialogic® CCS I/O Series 3 Card - EXS-7IO-1300/EXS-7IO-1300R

Description

The Dialogic® Common Channel Signaling I/O Series 3 card allows you to use one of the following cards in a distributed environment on a CSP:

• SS7 Series 3 card

• ISDN Series 3 card

• IP Signaling Series 3 card

The single slot CCS I/O Series 3 card is paired with one of the above cards to support either a single 10 Base-T or 100 Base-T Ethernet connection, auto-selected.

The Common Channel Signaling card call control at the Server Node matrix communicates with the CSP Matrix Series 3 Card on remote nodes over the Ethernet via the CCS I/O Series 3 card. A redundant CCS card connects to the remote matrix through the Ethernet, and to the primary SS7 Series 3 card, ISDN Series 3 card, or IP Signaling Series 3 card through the CCS I/O Series 3 Redundancy Link cable.

The CCS I/O Series 3 Redundancy Link cable serves as an independent link for redundancy between the adjacent CCS I/O Series 3 cards.

Important! Redundant configurations are optional. If selected, the removal of one of a pair of CCS I/O Series 3 cards will not interrupt CCS system operation nor require user intervention.

Placement

The CCS I/O Series 3 card resides in the rear card slot of a CSP 2090, CSP 2110 or CSP 2040 chassis directly behind the corresponding CCS card.

Configuration Information

The part number, serial number, model number, and revision are located on the back of the board.

Specifications

The CCS I/O Series 3 card is designed to the following electrical, physical and environmental specifications.

Electrical | Specification
--- | ---
Supply Voltage, Vcc | 5.00V
Supply Current, Vcc @ 5.0V | 0.74A (typical)

Physical | Specification
--- | ---
Height | 318.5 mm (12.54 in.)
Depth | 105.2 mm (4.14 in)
Width | 19.7 mm (0.775 in.)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) @ 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) @ 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 m (13,123 ft.)

Related Products

The products related to the CCS I/O Series 3 card are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
SS7 Series 3 Card | EXS-SS7-1360 | EXS-SS7-1360R
ISDN Series 3 Card | EXS-PRI-1300 | EXS-PRI-1300R
IP Call Server Card | EXS-SCS-1000 | EXS-SCS-1000R
CCS I/O Series 3 Redundancy Cable | EXS-CBL-1000 | EXS-CBL-1000R

Front and Side Views

The front view shows the LEDs, Redundancy Link connector and Ethernet connectors.

Controls and Indicators

The table below describes the LEDs as shown in the front view of the CCS I/O Series 3 card.

LEDs | Color/Status | Description
--- | --- | ---
Power | Green | Power is within acceptable limits.
Off | Power is not available or out of tolerance.
Activity | Green | CCS I/O Series 3 card is active.
Off | CCS I/O Series 3 card is inactive.
Redundancy Link Status | Green | High speed redundant link is active.
Off | High speed redundant link is inactive.
Port A | On (100 Base-T) | S-Speed
On (10 Base-T)
On | L-Link
Off
Blinking Green | A-Activity
Off
Port B (Reserved for future use) | On (100 Base-T) | S-Speed
On (10 Base-T)
On | L-Link
Off
Blinking Green | A-Activity
Off

CCS. Network architecture using SS7 protocol for the exchange of information between telecommunications nodes and networks on an out-of-band basis.
See Signaling System Number Seven.
See Integrated Services Digital Network.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
See Common Channel Signaling.
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."