You are here: CSP Developer’s Guide: Overview > 8 DSP Series 2 Cards Product Description > Supported Features

Supported Features

Features

The T.30 Fax suite supports the following enhanced Group 3 fax features:

• Resolutions: normal, fine, very fine

• Standard page width formats

• Conversion of document formats into different formats, resolutions, or encodings online (on-the-fly) or offline

• Encoding: 1D, 2D, and MMR

• Fax transmission or reception at rates up to 14,400 bps

• 12 simultaneous faxes per DSP chip (6 per stream)

• ITU Group 3 compliance for worldwide fax machine compatibility

• Document fax conversion (shrinking to fit A4, for example) to be supported "on the fly" via TLV

• Page format conversions: A3, A4, and B4

• Fax session and document status monitoring

• Fax queues

• FoIP (on the IP Signaling Series 3 card)

• Error Correction Mode (ECM)

• Permanent fax records (stored on the NFS server)

• Configurable per-card, per-chip, and per-call

• Digital signal processor (DSP)-based flexibility

• Transmit Page Range in TIFF File.

NOTE: This release does not support T.30 Polling Mode.

Bits Per Second
Digital Signal Processor
International Telecommunications Union (UN)
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.