0x0118 Companding Conversion Mode

Use this TLV to specify whether PCM encoding format conversion should be bypassed or not. The default is 0 in which case PCM encoding format is not bypassed. A value of 1 bypasses the conversion process and forces the B side of the call leg to use the A side’s companding format.

Used in:
0x1E and 0x001E Generic PPL ICBs in:
Route Control message
Connect with Data message

Byte | Description
0, 1 | Tag 0x0118
2, 3 | Length 0x0002
4, 5 | Value[0] 0x0000 Companding Conversion enabled (default) 0x0001 Companding Conversion disabled

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Pulse Code Modulation.
See Programmable Protocol Language.