L3P CIC PPL Event Indications (ANSI)

Event ID | Event
--- | ---
0x01 | Reset circuit success indication
0x08 | Remote maintenance block or maintenance group block indication
0x09 | Remote maintenance unblock or maintenance group unblock indication
0x0A | ACM received
0x0B | ANM received
0x0C | CPG received
0x0E | ISUP protocol violation
0x12 | Local maintenance block / group maintenance block success
0x13 | Local maintenance unblock / group maintenance unblock success
0x15 | Local circuit maintenance unblocking indication
0x16 | UCIC received
0x17 | No GRS/RSC Received, CICs In Service
0x26 | CRM received
0x63 | DSP Resource Allocation Failure

L3P CIC PPL Event Requests (ANSI)

Event ID | Event
--- | ---
0x01 | Send ACM
0x02 | Send CPG
0x03 | Send ANM
0x04 | Request local maintenance blocking (sends BLO)
0x05 | Request local maintenance group blocking (sends CGB)
0x06 | Request local maintenance unblocking (sends UBL)
0x07 | Request local maintenance group unblocking (sends CGU)
0x08 | Send GRS
0x09 | Send RSC
0x0C | Indicate CPC to wait for incoming COT report when continuity check is being performed on previous circuit.
0x0D | Send incoming continuity check report if continuity check was performed on previous circuit.
0x1F | Send CQM
0x24 | Send FAC
0x25 | Send PAM
0x2A | Send INR
0x2B | Send INF
0x2D | Send SUS
0x2E | Send RES
0x2F | Send CVT
0x31 | IAM Request with parameters
0x40 | Manual Stop
0x41 | Send Continuity Check Request Message (CCR)
0x45 | Send EXM
0x46 | Send FOT

See Integrated Services Digital Network User Part.
Digital Signal Processor
See Circuit Identification Codes.
See Programmable Protocol Language.
American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.
Continuity Check Request message (ISUP)