0x0648 Receive Resolution Type

Use this TLV in the Generic Card Configure (0x0122) message to set the Receive Resolution Type.

Byte | Description
0, 1 | Tag: 0x0648 Receive Resolution Type
2, 3 | Length: 0x0002
4, 5 | Value[0-1]: Resolutions to advertise in the DIS (bitmask) 0x0004 RES_204x98 0x0008 RES_204x196 0x0010 RES_204x391 0x0020 RES_408x391 0x0040 RES_200x200 0x0080 RES_300x300 0x0100 RES_400x400 0x01FC (default)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.