0x0004 Remove Matrix

Used in:
IP Signaling Series 3 Card Configure message (0x0100)

Byte | Description
0, 1 | Tag 0x0004
2, 3 | Length 0x0002
4 | Value[0] Call Server ID to be removed, MSB 0x00 To remove a specific Matrix 0xFF To remove all configured Matrices
5 | Value[1] Call Server ID to be removed, LSB 0x00-0x3F To remove a specific Matrix 0xFF To remove all configured Call Matrices

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Most Significant Bit
Least Significant Bit