0x2795 Destination RTP Port

Used in:
0x0033 NPDI Universal ICB in:
Request for Service with Data message
Route Control message
Outseize Control message

Byte | Description
0, 1 | Tag 0x2795 Destination RTP Port
2, 3 | Length 0x0004
4, 5 | Value[0, 1] 0x0000 (Do not change)
6, 7 | Value[2, 3] RTP Port

Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.
Outgoing call setup during real-time call processing on a specific channel.
Real-Time Transport Protocol. Supports transport of real-time data like interactive voice and video over packet-switched networks.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."